Joey Installation Help Notes.
---------------------------------
                                                                    
The installation and configuration of the Joey PC software is a
relatively simple procedure that can be divided into two simple
operations. The operations are

    1. Installation of the Joey software.
    2. Installation of the USB -> Serial device driver.

Both operations are discussed in detail below.

1. Installation of the Joey software.
-----------------------------------------

1.  Insert the Joey software CD into your computer.

2.  The setup process should start automatically via the autorun.inf
    file. If the setup/installation does not start automatically 
    within 10 to 15 seconds, perform one of the following two operations

        a. Open Windows Explorer, navigation to your CD ROM drive and
           double click on the Joeysetup_verX.X.X.exe file.

        b. Click Start/Run and enter d:\Joeysetup_verX.X.X.exe where d is
           the drive identifier on the PC you are installing the
           software.

3.  Follow the installation instructions carefully. YOu will be prompted
    to enter the location where you want to install the software and the
    location of where to store any icons. If you an unsure of the 
    locations it is suggested that you accept the defaults that are 
    suggested by the setup program.

4.  The software should now install properly.

5.  At the end of the installation procedure you will be prompted to
    reboot the computer. The computer must be rebooted before the 
    Joey software should be executed.


2. Installation of the USB -> Serial device driver.
---------------------------------------------------

Refer to the documents in the folder D:\Manual for detailed help
regarding the installation of the USB cable.  Further information
is listed below.

1.  Insert the USB download cable/dongle into your computers USB port.
    Please ensure that the cable/dongle is not connected to any TAG-A2 
    units at this moment.
 
2.  Windows should detect that new Hardware has been detected and 
    activate the New Hardware Wizard.

3.  Choose the option "Install from a list or specific location "
    (Advanced)". Select the next option.

4.  Select the "Search for the best driver in these locations". Enter
    the path d:\drivers where d is the drive identifier on the PC
    you are installing the software in the "Ïnclude this location in 
    the search location" via the BROWSE button.

5.  If the computer you are using has the Windows XP operating system
    installed and you receive a warning similar to "The software you
    are installing has not passed the Windows logo testing to verify
    its compatibility with Windows XP" select the "Continue Anyway"
    option.

6.  A confirmation screen should be given to indicate that the driver
    has been installed correctly. 

7.  The Joey PC software should now be fully installed and ready 
    for operation.



TROUBLE SHOOTING
----------------

If you are having trouble connecting to your TAG-J2 unit with the 
Joey software please take the follwoing steps.

1.  From the "Control Panel" on your computer select "System".

2.  Select the "Device Manager" option. This might be its own TAB
    or it could be under a "Hardware" tab.

3.  Select the "Universal Serial Bus Contorllers" and ensure that
    there is a "FTDI FT8UXX Device" driver installed
    under this option. If there is not please try and reinstall 
    the USB -> serial device driver as per the instructions in 
    section 2.

4.  When running the Joey software ensure that you have the 
    correct port selected. I.e. If you are using the USB cable then
    ensure that the USB option is selected in the Joey software.

5.  Consult your manual for further information regarding 
    connections.

6.  Contact your local Joey dealer.

